 input file
 - - - the numbers of meshes in x-,y-,z-directions
	4096	2560	1
 - - - threadx, thready, threadz
	16	16	1
 - - -  system size [m]
	10e-3
 - - -  boundary conditions for x, y, z (0:Neumann, 1:Mirror, 2:Periodic)
 	0	0	0
 - - -  maximum number of time step
	2204278
 - - - time constant ( 4.5 for 2D, 6.8 for 3D ) 
	4.5
 - - -  grain boundary energy [J/m2]
	0.79
 - - - prefactor and activation energy for grain boundary mobility
	6.2e-3	176e+3
 - - - type of temperature calculation
	3
 - - - parameters for temperature calculation
	298.15 6.0e3 40.0 4.0e-4 9e-6 -1.0e-3 -5.0e-3 0
 - - - melting&solidification calculation
	1
 - - - parameters for melting&solidification calculation
	1.0 1791 1765
 - - - parameters for melting&solidification calculation
	0.0 -0.001 0.0 0.0 0.001 0.0 20
 - - - pinning calculation
	1
 - - - parameters for pinning calculation
	3.3 1.0 1.0
 - - - parameters for pinning calculation
	4e-5 0.0 0.0 0.0 1765
 - - - parameters for pinning calculation
	1e-8 0.0 0e-28 0.0 
 - - - the maximum number of grains for APT algorithm (2D:5, 3D:6)
	5
 - - - interface thickness, WW/dx
	6.0
 - - - name of file for initial microstructure
	initial_microstructure_data.ini
 - - - the skip numbers of time and grids for snapshots 
	24000	2  2  1

